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	Document Type:
	Systematic Review Questionnaire

	Dates:
	Circulation date
	Closing date

	
	13/8/2026
	12/09/2026

	TC Secretary
	This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Jane Wainaina (jwainaina@kebs.go.ke)



The Kenya Bureau of Standards is in the process of reviewing the Kenya Standard(s) as detailed in the list of Kenya Standard(s) for Systematic Review.

We are therefore seeking views from potential users in respect of relevance and effectiveness of the standard(s) listed below in addressing current market needs, regulatory needs and scientific and technological development.  

The Standard(s) are available at the Kenya Bureau of Standards Information Centre.  Please tick (mark) and fill your preference of the listed option.  (If the spaces provided are not enough, please attach a separate sheet of paper).

Please indicate your choice out of the following 4 actions which you prefer to be taken on each of these Kenya Standards.
    
	No.
	Standard Number, 
Title and 
Scope
	Proposed Action (Tick one option as appropriate)
	Justification for revision, amendment, or withdrawal (cite the specific clauses and wording preferred)

	
	
	Confirmation 
	Revision 
	Amendment 
	Withdrawal 
	

	1. 
	KS 506:1994, Cotton dish cloths – Specification

Scope
Prescribes the requirements for cotton dish cloths.
	
	
	
	
	

	2. 
	KS ISO 9073-16:2007,    Nonwovens - Water penetration - Hydrostatic pressure

Scope
ISO 9073-16:2007 describes the hydrostatic pressure test that measures the resistance of nonwoven fabrics to the penetration of water under varied hydrostatic head pressures.

ISO 9073-16:2007 applies to any nonwoven fabrics which are intended for use as a barrier to the penetration of fluids.
	
	
	
	
	

	3. 
	KS ISO 9073-17:2008, Nonwovens - Water penetration - Spray impact

Scope
ISO 9073-17:2008 specifies a method for measuring the resistance of fabrics to the penetration of water by impact.

The water penetration (spray impact) test is applicable to fabrics that are expected to exhibit a degree of water resistance or water repellency.

The results obtained with this method depend on the water repellency of the fibres or the treatment applied to the finished material, as well as on the construction of the material.

	
	
	
	
	

	4. 
	KS ISO 9073-2:1995, Nonwovens – Thickness

Scope
Lays down methods for the determination of the thickness, when under a specific pressure, of normal and bulky nonwoven textiles.
	
	
	
	
	

	5. 
	KS ISO 9073-3:1989, Nonwovens - Tensile strength and elongation

Scope
This document specifies a test method for the determination of the breaking force and elongation of nonwovens using a strip method in conditioned or wet state. This test method describes two procedures, Option A (width of test specimen: 25 mm) and Option B (width of test specimen: 50 mm).

This document specifies methods using constant rate of specimen extension (CRE) tensile testers. Constant rate of loading (CRL) instruments is covered, for information, in ISO 2062:2009, Annex A, in recognition of the fact that these instruments are still in use and can be used by agreement.

	
	
	
	
	

	6. 
	KS ISO 9073-10:2003, Nonwovens - Lint and other particles generation

Scope
ISO 9073-10:2003 specifies a test method for measuring the linting of nonwovens in the dry state. It can also be applied to other textile materials.
	
	
	
	
	

	7. 
	KS ISO 11948-1:1996,   Urine-absorbing aids - Whole-product testing

Scope
Gives a method for determining the absorption capacity of the absorbent core of body-worn urine-absorbing aids.
	
	
	
	
	

	8. 
	KS ARS 1694:2021, Medical respirators – Specification

Scope
	
	
	
	
	

	9. 
	KS ISO 9073-4:2021, Nonwovens - Tear resistance by trapezoid procedure

Scope
This document specifies a method for the determination of tear resistance of nonwovens by the trapezoid method.
This document applies to nonwovens.

	
	
	
	
	

	10. 
	KS ISO 9073-9:2008, Nonwovens - Drapability including drape coefficient

Scope
ISO 9073-9:2008 specifies a test method that is used to determine the drape coefficient of fabrics (nonwovens, wovens and knitted fabrics).
	
	
	
	
	

	11. 
	KS 2925:2022, Textiles - Reusable sanitary towels - Specification, Second Edition

Scope
Specifies the requirements, sampling and test methods for reusable sanitary towels (including reusable panty liners) for external use.
	
	
	
	
	



Name and (of respondent) ………………………………………………          Position…………………

Signature: …………………………………………………….

On behalf of: ……………………………………………………………….        (Name of organization)

Date:	

NOTE: Absence of any reply or comments shall be deemed to be an acceptance of the proposal for confirmation and shall constitute an approval for confirmation vote. 
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