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	Document Type:
	Systematic Review Questionnaire

	Dates:
	Circulation date
	Closing date

	
	2026/08/26
	2026/09/25

	TC Secretary
	This form shall be filled, signed and returned to Kenya Bureau of Standards for the attention of Ken Oduor (oduork@kebs.go.ke)


The Kenya Bureau of Standards is in the process of reviewing the Kenya Standard(s) as detailed in the list of Kenya Standard(s) for Systematic Review.
We are therefore seeking views from potential users in respect of relevance and effectiveness of the standard(s) listed below in addressing current market needs, regulatory needs and scientific and technological development.
The Standard(s) are available at the Kenya Bureau of Standards Information Centre. Please tick (mark) and fill your preference of the listed option. (If the spaces provided are not enough, please attach a separate sheet of paper).
Please indicate your choice out of the following 4 actions which you prefer to be taken on each of these Kenya Standards.
	No.
	Standard Number, Title and scope
	Proposed Action (Tick one option as appropriate)
	Justification for revision, amendment, or withdrawal

	
	
	Confirmation
	Revision
	Amendment
	Withdrawal
	

	1
	KS 1394-1:2000 — Textile burning behaviour - Ease of ignition
Scope: Specifies a method for measuring the ease of ignition of vertically oriented textile fabrics intended for apparel, curtains and draperies, including single- and multi-component textile assemblies such as coated, quilted, multilayer and sandwich constructions.
	
	
	
	
	

	2
	KS 1435:1999 — Coated fabrics for shoes - Specification
Scope: Specifies requirements for two types of PVC coated fabrics intended for use as shoe uppers.
	
	
	
	
	

	3
	KS 1125-1:1992 — Carpet backing fabrics - Jute fabrics
Scope: Specifies requirements for jute fabrics used as carpet backing fabrics.
	
	
	
	
	

	4
	KS 2333:2011 — Hand woven table mats - Specification
Scope: Specifies requirements for hand woven table mats, including essential quality characteristics for materials, workmanship and finished product performance.
	
	
	
	
	

	5
	KS ISO 11378-1:2000 — Textile floor coverings - Laboratory soiling - Kappasoil test
Scope: Specifies a laboratory method for assessing the propensity of textile floor coverings to soiling using an artificial soil composition; the method may also be used to assess the efficiency of cleaning chemicals and cleaning equipment.
	
	
	
	
	

	6
	KS ISO 11377:1997 — Textile floor coverings - Floor soiling test site and evaluation
Scope: Specifies the procedure for setting up a test site for textile floor coverings and evaluating levels of soiling as measured by colour change.
	
	
	
	
	

	7
	KS 835-3:1988 — Textile floor coverings - Delamination strength of secondary backing
Scope: Specifies a method for determining the delamination strength of the secondary backing of textile floor coverings.
	
	
	
	
	

	8
	KS 835-2:1989 — Textile floor coverings - Constructional details
Scope: Specifies methods for determining constructional details of textile floor coverings.
	
	
	
	
	

	9
	KS 835-10:1997 — Textile floor coverings - Knot types of handmade carpets
Scope: Specifies a method for determining the types of knots used in handmade carpets.
	
	
	
	
	

	10
	KS 835-11:1997 — Textile floor coverings - Tuft length of hand knotted carpets
Scope: Specifies a method for determining the tuft length above the woven ground of hand-knotted carpets.
	
	
	
	
	

	11
	KS 1843:2005 — Carpet underlays - Specification
Scope: Specifies performance requirements for fibrous, non-fibrous and combined carpet underlays.
	
	
	
	
	

	12
	KS ISO 3018:1974 — Rectangular textile floor coverings - Dimensions
Scope: Specifies a method for determining the dimensions of rectangular textile floor coverings, both handmade and machine-made, having a length-to-width ratio of less than 5; it does not apply to materials laid edge-to-edge as tiles.
	
	
	
	
	

	13
	KS 779-3:2021 — Carpets - Part 3: Woven carpets
Scope: Specifies requirements for woven carpets.
	
	
	
	
	

	14
	KS ISO 1763:2020 — Textile floor coverings - Tufts/loops per unit area
Scope: Specifies a method for determining the number of tufts and/or loops per unit length and per unit area of textile floor coverings with pile consisting of tufts and/or loops.
	
	
	
	
	

	15
	KS ISO 1766:1999 — Textile floor coverings - Pile thickness
Scope: Specifies a method for determining the thickness of pile above the substrate of a textile floor covering; applicable to pile capable of being shorn from the substrate, with separate measurement where pile thickness or density varies.
	
	
	
	
	

	16
	KS ISO 8543:2020 — Textile floor coverings - Mass determination
Scope: Specifies methods for determining total mass per unit area, total pile mass per unit area and mass of pile per unit area above the substrate, and for calculating measured surface pile density and measured pile fibre volume ratio.
	
	
	
	
	

	17
	KS ISO 3018:1974 — Textile floor coverings - Dimensions
Scope: Specifies a method for determining the dimensions of rectangular textile floor coverings, both handmade and machine-made, having a length-to-width ratio of less than 5; it does not apply to materials laid edge-to-edge as tiles.
	
	
	
	
	

	18
	KS ISO 4919:2012 — Carpets - Tuft withdrawal force
Scope: Specifies a method for determining tuft withdrawal force and applies to carpets with cut or loop pile yarn structures.
	
	
	
	
	

	19
	KS ISO 2094:1999 — Textile floor coverings - Thickness loss under dynamic loading
Scope: Specifies a method for determining thickness loss of textile floor coverings under dynamic loading; applies to floor coverings with a surface level in height and construction, with different areas tested separately where necessary.
	
	
	
	
	

	20
	KS ISO 2551:2020 — Textile floor coverings - Dimensional changes due to water and heat
Scope: Specifies a procedure for determining dimensional changes and distortion out of plane likely to occur when textile floor coverings and textile floor coverings in tile form are subjected to varied water and heat conditions.
	
	
	
	
	

	21
	KS ISO 10361:2015 — Textile floor coverings - Appearance changes by Vettermann drum
Scope: Describes laboratory methods using the Vettermann drum and hexapod tumbler tester to produce changes in appearance of textile floor covering specimens for assessment.
	
	
	
	
	

	22
	KS ISO 1765:1986 — Machine-made textile floor coverings - Thickness
Scope: Specifies a basic method for determining the thickness of machine-made textile floor coverings; where areas differ in thickness or construction, they should be tested separately where possible.
	
	
	
	
	

	23
	KS ISO 9405:2015 — Textile floor coverings - Assessment of changes in appearance
Scope: Describes procedures for assessing overall changes in appearance of textile floor coverings caused by Vettermann drum and hexapod tumbler testers.
	
	
	
	
	

	24
	KS ISO 2424:2007 — Textile floor coverings - Vocabulary
Scope: Gives definitions of terms relating to textile floor coverings and defines categories of these products.
	
	
	
	
	

	25
	KS 779-2:2022 — Carpets - Part 2: Sisal carpets
Scope: Specifies requirements for sisal carpets woven without pile.
	
	
	
	
	

	26
	KS ISO 24342:2018 — Textile floor coverings - Side length and squareness
Scope: Describes methods for determining side length, edge straightness and squareness of resilient or textile floor tiles and planks.
	
	
	
	
	



Name and (of respondent) ………………………………………………          Position…………………

Signature: …………………………………………………….

On behalf of: ……………………………………………………………….        (Name of organization)

Date:	

NOTE: Absence of any reply or comments shall be deemed to be an acceptance of the proposal for confirmation and shall constitute an approval for confirmation vote. 
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